Cutting # [17]	Date: 16.V.86	(y) [16] to (y) [17] = 1.67m.

Widths:	Heights: 15A. Cheek width at (X):

L 0.125 (broken)

1. N/A	6. R N/A L N/A R 0.085

2. 1.12?*	7. R N/A L N/A

3. 0.40?*	8. R N/A L N/A

4. 0.345 (from traces)	9. R 0.82 L N/A

5. 0.55 (Left side broken) 9A. R: 0.73

3A. 0.355 (Y - R; x 2) = 0.71

BL2 to top of 3rd course = 0.30

Profile Cross-Sections (depths in centimeters) Up----------------BL----------Down BL to bottom of cutting: N/A

10	10	10	10	10	10

11*

beginning of top of 3rd course:	edge

3	join

42	42.5	39	37	32.5	28.5	26	24	22.5	22	21.5	20.5	20.5	21	21	21	21.5 (BL2) 22	23	24
25	28	33	38.5	41	44	44	46	join	Total height = 0.58m.	4th course – beginning:	2	37	39	breaks--

13

Top = 0.435m. at 0.4 down from top of course	Intermediate to top = 0.26 at 0.18 from top of course
Middle = 0.21at (BL2)	Intermediate to bottom = 0.30 at 0.47 from top of course
Bottom = 0.43 at 0.58 from top of course

Remarks: * #2: *Measured from semi-inaccurate (y)- line.

#3: L side of stem broken – I measured to traces further back into the cutting.

#4: R side of stem broken.

#11: Subtract 0.05 from every measurement from 3rd course down.

X calculated – 0.335 down from top of 3rd course (taken from [15]).